

12345 College Blvd. Overland Park, KS 66210-1299

***Sean Bergman, Director of Operations***

Email: [sbergman@jccc.edu](mailto:sbergman@jccc.edu) 913-469-2535 (Office) 913-469-2566 (Fax)

GENERAL SPECIFICATIONS – POLSKY THEATRE

|  |  |  |
| --- | --- | --- |
| Polsky Theatre is the medium-sized venue of the three theatres within the Midwest Trust Center at Johnson County Community College, with a total seating capacity of 424 located on two levels. The Orchestra is on the lower level. The tier and boxes are on the upper level. The farthest seat from the stage is 50 feet. It is a semi-thrust stage, jutting into the house, partially surrounded on three sides.  It is designed for the spoken voice, and therefore lends itself to the staging of drama performances. It is equipped with a LARES Acoustic Enhancement System for acoustic music. | **STAGE SURFACE**  Stage floor (thrust) is constructed in 3'×6' ¾" Plyron decking resting on Stage Right Company’s assembly of platforming. **USE OF ROSIN IS PROHIBITED IN THE MIDWEST TRUST CENTER.**  **DANCE FLOOR**  Polsky Theatre has a Rosco dance floor for ballet and modern dance. It is two-sided, black/gray. There are 6 sections, each 5' 4" wide and 40' long. In addition, there are custom-cut sections to fit the thrust stage of the Theatre. | **SOFTGOODS**  *Type* Quantity  Color Size W×H  *Grand Drape* one Blue 54'×25'  *Grand Teaser* one Blue 81'×8'  *Midstage Traveller* one Black 54'×25'  *Legs* three  Black 18'×28'  *Borders* three  Black 81'×8'  *Cyclorama* one White 52'×29'  *Scrim* one  Black 54'×30'  **LOADING DOCK**   * 4' - 0" height (dock plate avail) * Door 11' 11" wide, 9' 3" high |
| It is equipped with 39 linesets, including 2 devoted electrics with the capacity for more with the use of drop boxes. The stage is on the same level as house doors and house divide for easy access. | **RIGGING**  Counterweight system: single purchase lines.  39 linesets |
|  | Devoted linesets: |
| **STAGE MEASUREMENTS** | * 2 Electrics |
| * Proscenium Width: 36' * Proscenium Height: 25' * Wall to wall: 70' 6" * Plaster line to upstage wall: 32' * Plaster line to downstage edge of apron: 14' 6" * Grid height: 51' * Fly rail is stage left * Loading rail: (2) 1 @ 24', 1 @ 48' * System pipe out trim: 44' 3" | * 1 Grand Drape * 1 Grand Teaser * 1 Mid-stage Traveller   Length of battens: 54' Capacity: 25 lb. per foot Average distance between  linesets: 9" Maximum high trim: 45' |

# HEADSETS AND COMMUNICATIONS

#### PAGING SYSTEM:

Access at stage right Production Control Panel and in Control Booth. Can access dressing rooms, Green Room and all support areas.

#### MONITOR SYSTEM:

All dressing rooms and Green Room receive assignable video and audio feeds from the Stage.

# DRESSING ROOMS

#### Stage/ground level:

**Room 192:** services 3-4 people

**Room 196:** services 5-7 people

**Room 198:** services 10-15 people

#### Second floor:

**Room 292:** services 15-20 people

**Room 294:** services 3-4 people

**Room 298:** services 20-25 people

All dressing rooms are equipped with lighted, dimmable makeup mirrors, toilets and showers.

# MUSICAL EQUIPMENT

* Steinway Model D 9' Concert Grand
* Baldwin 9' Concert Grand
* Kawai Baby Grand
* Musician chairs: 100
* Music stands: 100
* Music stand lights: 77
* Choral risers: 7, 4-tier
* Band risers: 16 4'×8' Wenger platforms

at 8", 12", 16", 24", 32" or 40"

* Conductor’s podiums

# SPECIAL EFFECTS EQUIPMENT

* Mirror ball with rotator
* 2 DF-50 Hazers
* 2 Rosco Delta 3000 foggers

**MIDWEST TRUST CENTER PRODUCTION STAFF**

**Technical Director *Sean Bergman*** 913-469-2535

[sbergman@jccc.edu](mailto:sbergman@jccc.edu)

## Master Electrician

### Tripp McMillan

913-469-8500, ext. 3995

[tmcmilla@jccc.edu](mailto:tmcmilla@jccc.edu)

## Head Audio Engineer

### Ian Mason

913-469-8500, ext. 3291

[imason@jccc.edu](mailto:imason@jccc.edu)

## Technical Director

### Anthony Putzier

913-469-8500, ext. 3768

[aputzier@jccc.edu](mailto:aputzier@jccc.edu)

**Main College Number** 913-469-8500

**Fax** 913-469-2566