

12345 College Blvd. Overland Park, KS 66210-1299

##### Sean Bergman, Director of Operations

Email: sbergman@jccc.edu 913-469-2535 (Office)

GENERAL SPECIFICATIONS – YARDLEY HALL

|  |  |  |
| --- | --- | --- |
| Yardley Hall is the largest of the three theatres in the Midwest Trust Center at Johnson County Community College. Its total seating capacity of 1,341 is divided on four levels: Orchestra, Tier, Balcony and Box. The farthest seat from the stage is approximately 130 feet, creating a unique feeling of intimacy for a house of this size. It is equipped with 41 linesets, with 2 devoted electrics, and capacity for more with the use of drop boxes.An acoustical shell is available for orchestral events. One half of the apron is a screw-jack lift that can be used to pit orchestras.Yardley Hall is ideal for dance or music. The acoustics are excellent, and can be tuned for voice or music. | **LOADING DOCK*** 4' - 0" height
* Door 11' 11" wide, 9' 3" high
* Dock plate available
* Dock size: 64' × 11' 9"

**STAGE SURFACE****SCREWING INTO THE STAGE SURFACE IS PROHIBITED.**Stage floor is flat and even. Top surface is 3/4" oak hardwood. Supporting structure top to bottom:* Oak hardwood
* 3/4" plywood
* 1 1/8" plywood
* 2 × 4 sleeper
* 14 gauge steel sheet
 | Devoted Linesets:* 2 electrics
* 3 orchestra ceiling pieces
* 1 Grand Drape
* 1 Grand Teaser
* 1 Midstage Traveller Length of battens: 77' Capacity: 25 lb. per foot System pipeout trim: 66'
* Average distance between linesets: 9"
* Plaster line to first lineset: 1' 5"
* Plaster line to last lineset: 37'
* Maximum high trim: 66'

**SOFTGOODS***Type* QuantityColor Size W×H |
| **STAGE MEASUREMENTS*** Proscenium Width: 55'
* Proscenium Height: 32'
* Wall to wall: 133', 99' of stage floor
* Center stage to S.R. wall: 60', (49' 6" of stage floor)
* Center stage to S.L. wall: 73', (49' 6" of stage floor)
* Plaster line to upstage wall: 38' 4"
* Plaster line to edge of apron: 21' (with pit raised)
* Plaster line to edge of apron: 9' (with pit down)
* Grid height: 72'
* Fly rail is stage right
* Loading rail: (2) 1 @ 66', 1 @ 58'
 | **USE OF ROSIN IS PROHIBITED IN THE MIDWEST TRUST CENTER.****DANCE FLOOR**Yardley Hall has black and gray Harlequin dance floors for ballet and modern dance. There are 6 sections, each are 6' 6" wide and 48' long.**RIGGING**Counterweight system: single purchase lines, 41 linesets*(See lighting spec. sheet, page 2, for further detail)* | *Grand Drape* one Burgundy 70'×32'*Grand Teaser* one Burgundy 124'×12'*Midstage Traveller* one Black velour 70'×32'*Legs* fourBlack velour 20'×32'*Borders* fourBlack velour 124'×12'*Cyclorama* one White 75'×45'*Scrim* oneBlack 50'×25'*Full Stage* four panelsBlack 20'×32' ea. |
|  |  | *Leno*White |

# HEADSETS AND COMMUNICATIONS

#### CLEARCOM SYSTEM:

* 8 wired headsets with beltpacks
* 4 wireless units

#### PAGING SYSTEM:

Access at stage right Production Control Panel and in Control Booth. Can access dressing rooms, Green Room and all support areas.

#### MONITOR SYSTEM:

All dressing rooms and Green Room receive assignable video and audio feeds from the Stage.

# ORCHESTRA SHELL

Yardley Hall has a removable, wooden orchestra shell which is stored upstage left on the stage floor when not in use. The dimensions are:

* Downstage width: 55'
* Upstage width: 32'
* Downstage height: 32'
* Upstage height: 28.25'

The ceiling of the shell is equipped with 44 Cine Queens at 1000w each. Use of the grand drape is not possible with the shell in place.

# DRESSING ROOMS

Because the Center is a multi-venue facility, MIdwest Trust Center Operations determines dressing room assignments.

##### Stage/ground level:

**Room 192:** services 3-4 people

**Room 196:** services 5-7 people

**Room 198:** services 10-15 people

##### Second floor:

**Room 292:** services 15-20 people

**Room 294:** services 3-4 people

**Room 298:** services 20-25 people

All dressing rooms are equipped with lighted, dimmable makeup mirrors, toilets and showers.

# MUSICAL EQUIPMENT

* Steinway Model D 9' Concert Grand
* Baldwin 9' Concert Grand
* Kawai Baby Grand
* Musician chairs - 100
* Music stands - 100
* Music stand lights - 77
* Choral risers
* Band risers: 16 – 4' × 8' Wenger platforms

at 8", 12", 16", 24", 32" or 40"

* Conductor’s podiums

# SPECIAL EFFECTS EQUIPMENT

* 2 Rosco Delta 3000 foggers
* 2 DF-50 Hazers
* Mirror ball with rotator

**MIDWEST TRUST CENTER PRODUCTION STAFF**

## Director of Operations

### Sean Bergman

913-469-2535

sbergman@jccc.edu

## Technical Director

### Anthony Putzier

913-469-8500 ext. 3768

aputzier@jccc.edu

## Master Electrician

### Tripp McMillan

913-469-8500, ext. 3995

tmcmilla@jccc.edu

## Head Audio Engineer

### Ian Mason

913-469-8500, ext. 3291

imason@jccc.edu

**Main College Number** 913-469-8500

**Fax** 913-469-2566