

12345 College Blvd. Overland Park, KS 66210-1299

##### Sean Bergman, Director of Operations

Email: [sbergman@jccc.edu](mailto:sbergman@jccc.edu) 913-469-2535 (Office)

GENERAL SPECIFICATIONS – YARDLEY HALL

|  |  |  |
| --- | --- | --- |
| Yardley Hall is the largest of the three theatres in the Midwest Trust Center at Johnson County Community College. Its total seating capacity of 1,341 is divided on four levels: Orchestra, Tier, Balcony and Box. The farthest seat from the stage is approximately 130 feet, creating a unique feeling of intimacy for a house of this size. It is equipped with 41 linesets, with 2 devoted electrics, and capacity for more with the use of drop boxes.  An acoustical shell is available for orchestral events. One half of the apron is a screw-jack lift that can be used to pit orchestras.  Yardley Hall is ideal for dance or music. The acoustics are excellent, and can be tuned for voice or music. | **LOADING DOCK**   * 4' - 0" height * Door 11' 11" wide, 9' 3" high * Dock plate available * Dock size: 64' × 11' 9"   **STAGE SURFACE**  **SCREWING INTO THE STAGE SURFACE IS PROHIBITED.**  Stage floor is flat and even. Top surface is 3/4" oak hardwood. Supporting structure top to bottom:   * Oak hardwood * 3/4" plywood * 1 1/8" plywood * 2 × 4 sleeper * 14 gauge steel sheet | Devoted Linesets:   * 2 electrics * 3 orchestra ceiling pieces * 1 Grand Drape * 1 Grand Teaser * 1 Midstage Traveller Length of battens: 77' Capacity: 25 lb. per foot System pipeout trim: 66' * Average distance between linesets: 9" * Plaster line to first lineset: 1' 5" * Plaster line to last lineset: 37' * Maximum high trim: 66'   **SOFTGOODS**  *Type* Quantity  Color Size W×H |
| **STAGE MEASUREMENTS**   * Proscenium Width: 55' * Proscenium Height: 32' * Wall to wall: 133', 99' of stage floor * Center stage to S.R. wall: 60', (49' 6" of stage floor) * Center stage to S.L. wall: 73', (49' 6" of stage floor) * Plaster line to upstage wall: 38' 4" * Plaster line to edge of apron: 21' (with pit raised) * Plaster line to edge of apron: 9' (with pit down) * Grid height: 72' * Fly rail is stage right * Loading rail: (2) 1 @ 66', 1 @ 58' | **USE OF ROSIN IS PROHIBITED IN THE MIDWEST TRUST CENTER.**  **DANCE FLOOR**  Yardley Hall has black and gray Harlequin dance floors for ballet and modern dance. There are 6 sections, each are 6' 6" wide and 48' long.  **RIGGING**  Counterweight system: single purchase lines, 41 linesets  *(See lighting spec. sheet, page 2, for further detail)* | *Grand Drape* one Burgundy 70'×32'  *Grand Teaser* one Burgundy 124'×12'  *Midstage Traveller* one Black velour 70'×32'  *Legs* four  Black velour 20'×32'  *Borders* four  Black velour 124'×12'  *Cyclorama* one White 75'×45'  *Scrim* one  Black 50'×25'  *Full Stage* four panels  Black 20'×32' ea. |
|  |  | *Leno*  White |

# HEADSETS AND COMMUNICATIONS

#### CLEARCOM SYSTEM:

* 8 wired headsets with beltpacks
* 4 wireless units

#### PAGING SYSTEM:

Access at stage right Production Control Panel and in Control Booth. Can access dressing rooms, Green Room and all support areas.

#### MONITOR SYSTEM:

All dressing rooms and Green Room receive assignable video and audio feeds from the Stage.

# ORCHESTRA SHELL

Yardley Hall has a removable, wooden orchestra shell which is stored upstage left on the stage floor when not in use. The dimensions are:

* Downstage width: 55'
* Upstage width: 32'
* Downstage height: 32'
* Upstage height: 28.25'

The ceiling of the shell is equipped with 44 Cine Queens at 1000w each. Use of the grand drape is not possible with the shell in place.

# DRESSING ROOMS

Because the Center is a multi-venue facility, MIdwest Trust Center Operations determines dressing room assignments.

##### Stage/ground level:

**Room 192:** services 3-4 people

**Room 196:** services 5-7 people

**Room 198:** services 10-15 people

##### Second floor:

**Room 292:** services 15-20 people

**Room 294:** services 3-4 people

**Room 298:** services 20-25 people

All dressing rooms are equipped with lighted, dimmable makeup mirrors, toilets and showers.

# MUSICAL EQUIPMENT

* Steinway Model D 9' Concert Grand
* Baldwin 9' Concert Grand
* Kawai Baby Grand
* Musician chairs - 100
* Music stands - 100
* Music stand lights - 77
* Choral risers
* Band risers: 16 – 4' × 8' Wenger platforms

at 8", 12", 16", 24", 32" or 40"

* Conductor’s podiums

# SPECIAL EFFECTS EQUIPMENT

* 2 Rosco Delta 3000 foggers
* 2 DF-50 Hazers
* Mirror ball with rotator

**MIDWEST TRUST CENTER PRODUCTION STAFF**

## Director of Operations

### Sean Bergman

913-469-2535

[sbergman@jccc.edu](mailto:sbergman@jccc.edu)

## Technical Director

### Anthony Putzier

913-469-8500 ext. 3768

[aputzier@jccc.edu](mailto:aputzier@jccc.edu)

## Master Electrician

### Tripp McMillan

913-469-8500, ext. 3995

[tmcmilla@jccc.edu](mailto:tmcmilla@jccc.edu)

## Head Audio Engineer

### Ian Mason

913-469-8500, ext. 3291

[imason@jccc.edu](mailto:imason@jccc.edu)

**Main College Number** 913-469-8500

**Fax** 913-469-2566